IP ADDRESSING &OPENING INTERFACES

On FRS go to global mode means 3rd mode and write there int fa0/0 and then enter, give here ip for example, write here
Ip add 20.1.1.100 255.0.0.0 and then enter. Then write here no shut and then enter.
Then write here int s0/0 enter. Write here 4 commands (1) no shut (2)enca hdlc (3)clo rat 64000 (4)ip add 1.1.1.2 255.0.0.0
Then write here int s0/1 enter. Write here 4 commands (1) no shut (2)enca hdlc (3)clo rat 64000 (4)ip add 2.1.1.1 255.0.0.0

Now cum on R1 2interfaces connected directly (1) fa0/0 (2) s0/0
On R1 go to global mode means 3rd mode and write there. Int fa0/0 and then enter, give here ip for example, write here
Ip add 10.1.1.100 255.0.0.0 and then enter. Then write here no shut and then enter.
Then write here int s0/0 enter. Write here 4 commands (1) no shut (2)enca hdlc (3)clo rat 64000 (4)ip add 1.1.1.1 255.0.0.0

Now cum on R2 go to global mode means 3rd mode and write there. Int fa0/0 and then enter, give here ip for example, write here
Ip add 30.1.1.100 255.0.0.0 and then enter. Then write here no shut and then enter.
Then write here int s0/0 enter. Write here 4 commands (1) no shut (2)enca hdlc (3)clo rat 64000 (4)ip add 2.1.1.2 255.0.0.0

Now your topology is ready with ip's and u will see your all interfaces are up.

                                             
                                                            RIP ROUTING

ON FRS CUM ON 3RD MODE AND WRITE,ROUTER RIP ENTER.THEN WRITE HERE NETWORK 20.0.0.0 ENTER.THEN AGAIN WRITE NETWORK 2.0.0.0 ENTER.THEN AGAIN WRITE 1.0.0.0 ENTER.

ON R1 CUM ON 3RD MODE  AND WRITE ROUTER RIP ENTER.THEN WRITE HERE NETWORK 10.0.0.0 ENTER.THEN AGAIN WRITE NETWORK 1.0.0.0 ENTER.

ON R2 CUM ON 3RD MODE AND WRITE  ROUTER RIP ENTER.THEN WRITE HERE NETWORK 30.0.0.0 ENTER.THEN AGAIN WRITE NETWORK 2.0.0.0 ENTER.

NOW YOUR RIP ROUTING IS COMPLETE

                                 PASSWORDS
 TELNET PASSWORD
ON 3RD MODE WRITE. LINE VTY 0 4ENTER.THEN WRITE LOGIN ENTER.THEN WRITE PASSWORD CISCO (AUR WHAT U WANT TO KEEP) ENTER.

CONSOLE PASSWORD
ON 3RD MODE WRITE.LINE CON 0ENTER.THEN WRITE PASSWORD CISCO (AUR WHAT U WANT TO KEEP) ENTER.THEN WRITE LOGIN ENTER.

ENABLE MODE PASSWORD
ON 3RD MODE WRITE.ENABLE PASSWORD CISCO (AUR WHAT YOU WANT TO KEEP) ENTER.

ATTENTION#THESE PASSWORDS ARE NOT ENCRYPTED U HAVE TO ENCRYPT MANUALLY.FOR SEE THESE PASSWORDS BEFORE DOING ENCRYPTION CUM ON 2ND MODE AND WRITE.SHOW RUNNING CONFIG ENTER.YOU WILL SEE ALL PASSWORDS AND OTHER CONFIGURATION HERE.

FOR PASSWORD ENCRYPTION

CUM ON 3RD MODE AND WRITE.SERVICE PASSWORD-ENCRYPTION ENTER.THEN 1 BY 1 WRITE ALL PASSWORDS HERE FOR EXAMPLE.
(1)ENABLE PASSWORD CISCO ENTER.
(2)LINE CON 0 ENTER
     PASSWORD CISCO ENTER
    LOGIN ENTER.
(2)LINE VTY 0 4 ENTER
     LOGIN ENTER
     PASSWORD CISCO ENTER.

NOW U CAN ACCESS YOUR ROUTERS.